**Draper® Shows Tailored AV Mounting Solutions at InfoComm 2019**

**(Spiceland, Ind.) –** In the world of LED video walls, each manufacturer requires a unique mounting solution. At InfoComm 2019, June 12-14 in Orlando, Draper will showcase its work with manufacturing partners to develop two such tailored mounting solutions

Draper partnered with Leyard and Planar to design an LED mounting solution for the Leyard® TVF Series video wall. Draper’s ADA-compliant solution features independent X-Y-Z adjustments for fast and flawless installation. Native 16:9 HD sizes include 5 x 5 (137" D), 6 x 6 (164" D), 8 x 8 (219" D), and more. Custom sizes and aspect ratios are available using the same design. This tailored mounting solution is for flat video walls.

There will be a curved solution on display. Draper worked with Absen to develop a tailored mounting solution for the Acclaim series LED panels. The Acclaim series has pixel pitches available from 1.2 to 3.8 in a true 16:9 aspect ratio. Draper’s solution provides a faceted curved array through precise alignment between each column of panels. This complete solution is provided with all needed hardware including side cladding and lower ventilated filler panels. It can also be tailored for flying applications and is easily adaptable to other manufacturers’ products.

To see these examples of Draper’s tailored AV mounting solutions developed in partnership with manufacturing partners, visit Draper in booth 1342 at InfoComm 2019, June 12-14 in Orlando.

**ABOUT DRAPER:**

Draper, Inc. creates core and tailored solutions for the professional audiovisual marketplace, including projection screens, custom AV structures, supports, enclosures and lifts, as well as window shades and video conferencing solutions.

Established in 1902, Draper markets through a network of dealers and distributors to the commercial, architectural, education and residential markets.

**Media Contact:**Terry Coffey

Phone: 765-856-1230

E-mail: **tcoffey@draperinc.com**

Website: **www.draperinc.com**